**SPRINT 4**

|  |  |
| --- | --- |
| Date | 14 December 2022 |
| Team ID | PNT2022TMID08806 |
| Project Name | Hazardous Area Monitoring for Industrial Plant powered by IoT |

**WOKWI CODE:**

#include <WiFi.h>//library for wifi

#include <PubSubClient.h>//library for MQtt

#include "DHT.h"// Library for dht11

#define DHTPIN 15 // what pin we're connected to

#define DHTTYPE DHT22 // define type of sensor DHT 11 #define LED 2

DHT dht (DHTPIN, DHTTYPE);// creating the instance by passing pin and typr of dht connected

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength);

//-------credentials of IBM Accounts------

#define ORG "iagqzu"//IBM ORGANITION ID

#define DEVICE\_TYPE "Deepak"//Device type mentioned in ibm watson IOT Platform

#define DEVICE\_ID "123"//Device ID mentioned in ibm watson IOT Platform

#define TOKEN "12345678" //Token String data3; float h, t;

//-------- Customise the above values --------

char server[] = ORG ".messaging.internetofthings.ibmcloud.com";// Server Name char publishTopic[] = "iot-2/evt/Data/fmt/json";// topic name and type of event perform and format in which data to be send

char subscribetopic[] = "iot-2/cmd/command/fmt/String";// cmd REPRESENT command type AND COMMAND IS TEST OF FORMAT STRING char authMethod[] = "use-token-auth";// authentication method char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;//client id

// -

WiFiClient wifiClient; // creating the instance for wificlient

PubSubClient client(server, 1883, callback ,wifiClient); //calling the predefined client id by passing parameter like server id,portand wificredential

void setup()// configureing the ESP32

{

**Serial**.begin(115200);

dht.begin(); pinMode(LED,OUTPUT); delay(10); **Serial**.println(); wificonnect(); mqttconnect();

}

void loop()// Recursive Function

{

h = dht.readHumidity(); t = dht.readTemperature();

**Serial**.print("temp:");

**Serial**.println(t);

**Serial**.print("Humid:");

**Serial**.println(h);

PublishData(t, h); delay(1000); if (!client.loop()) {

mqttconnect();

}

}

/\*.....................................retrieving to

Cloud. ............................. \*/

void PublishData(float temp, float humid) {

mqttconnect();//function call for connecting to ibm

/\* creating the String in in form JSon to update the data to ibm cloud

\*/

String payload = "{\"temp\":"; payload += temp; payload += "," "\"Humid\":"; payload += humid; payload += "}";

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish ok");// if it sucessfully upload data on the cloud then it will print publish ok in Serial monitor or else it will print publish failed

} else {

**Serial**.println("Publish failed");

}

}

void mqttconnect() {

if (!client.connected()) {

**Serial**.print("Reconnecting client to "); **Serial**.println(server);

while (!!!client.connect(clientId, authMethod, token)) { **Serial**.print("."); delay(500);

}

initManagedDevice(); **Serial**.println();

} } void wificonnect() //function defination for wificonnect

{

**Serial**.println();

**Serial**.print("Connecting to ");

WiFi.begin("Wokwi-GUEST", "", 6);//passing the wifi credentials to establish the connection

while (WiFi.status() != WL\_CONNECTED) {

delay(500);

**Serial**.print("."); }

**Serial**.println("");

**Serial**.println("WiFi connected");

**Serial**.println("IP address: ");

**Serial**.println(WiFi.localIP());

}

void initManagedDevice() {

if (client.subscribe(subscribetopic)) {

**Serial**.println((subscribetopic));

**Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED"); }

}

void callback(char\* subscribetopic, byte\* payload, unsigned int payloadLength)

{

**Serial**.print("callback invoked for topic: "); **Serial**.println(subscribetopic);

for (int i = 0; i < payloadLength; i++) { //Serial.print((char)payload[i]); data3 += (char)payload[i];

}


**Serial**.println("data: "+ data3); if(data3=="lighton") { **Serial**.println(data3); digitalWrite(LED,HIGH); } else

{ **Serial**.println(data3); digitalWrite(LED,LOW);

} data3="";


}

**WOKWI OUTPUT:**




**IBM WATSON PLATFORM** ➔

**DEVICE EVENT LOG:**



**DEVICE EVENT PAYLOAD:**



**DEVICE- BOARD:**

